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	LEAD AND COPPER

	Contaminant
(Units)

	Action
Level (AL)   
	90th
percentile
sample value 
	Range of tap sampling results
	Date
	# of sites
above
AL
	Action Level Exceedance YES/NO
	Likely Source of 
Contamination
	Health Effects of Contaminant


	Copper
(ppm)
	1.3
	[bookmark: Text70]     .061
	
	11/2024
	0
	No
	Corrosion of household plumbing systems; erosion of natural deposits; leaching from wood preservatives
	Copper is an essential nutrient, but some people who drink water containing copper in excess of the action level over a relatively short amount of time could experience gastrointestinal distress. Some people who drink water containing copper in excess of the action level over many years could suffer liver or kidney damage. People with Wilson’s Disease should consult their personal doctor.

	Lead
(ppb)
	15
	.004
	
	11/2024
	0
	No
	Corrosion of household plumbing systems, erosion of natural deposits
	(15 ppb in more than 5%) Infants and young children are typically more vulnerable to lead in drinking water than the general population. It is possible that lead levels at your home may be higher than at other homes in the community as a result of materials used in your home’s plumbing. If you are concerned about elevated lead levels in your home’s water, you may wish to have your water tested and flush your tap for 30 seconds to 2 minutes before using tap water. Additional information is available from the Safe Drinking Water Hotline (800-426-4791). 
(Above 15 ppb) Infants and children who drink water containing lead in excess of the action level could experience delays in their physical or mental development. Children could show slight deficits in attention span and learning abilities. Adults who drink this water over many years could develop kidney problems or high blood pressure.




	DETECTED WATER QUALITY RESULTS

	Microbiological Contaminants

	Contaminant
(Units)
	Level
Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of
Contamination
	Health Effects of Contaminant

	Turbidity
(NTU)
	.035
	2025
	TT
	N/A
	No
	Soil runoff
	Turbidity has no health effects. However, turbidity can interfere with disinfection and provide a medium for microbial growth. Turbidity may indicate the presence of disease-causing organisms. These organisms include bacteria, viruses, and parasites that can cause symptoms such as nausea, cramps, diarrhea, and associated headaches.

	

	Contaminant
(Units)
	Level
Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of
Contamination
	Health Effects of Contaminant

	Barium
(ppm)
	     
.0107
	2025
	2
	2
	No
	Discharge of drilling wastes; discharge from metal refineries; erosion of natural deposits
	Some people who drink water containing barium in excess of the MCL over many years could experience an increase in their blood pressure.

	Contaminant
(Units)
	Level
Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of
Contamination
	Health Effects of Contaminant

	Chlorine
(ppm)
	     
.30-1.6
	2025
	MRDL= 4
	MRDLG= 4
	No
	Water additive used to control microbes

	Some people who use water containing chlorine well in excess of the MRDL could experience irritating effects to their eyes and nose. Some people who drink water containing chlorine well in excess of the MRDL could experience stomach discomfort.

	Fluoride
(ppm)
	     
.69
	2025
	4.0
	4.0
	No
	Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories
	Some people who drink water containing fluoride in excess of the MCL over many years could get bone disease, including pain and tenderness of the bones. Fluoride in drinking water at half the MCL or more may cause mottling of children’s teeth, usually in children less than nine years old. Mottling, also known as dental fluorosis, may include brown staining and/or pitting of the teeth, and occurs only in developing teeth before they erupt from the gums.

	Contaminant
(Units)
	Level
Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of
Contamination
	Health Effects of Contaminant

	Nitrate
(as Nitrogen)
(ppm)
	     
.58
	2025
	10
	10
	     No
	Runoff from fertilizer use; leaching from septic tanks, sewage; erosion of natural deposits
	(5 ppm through 10ppm) Nitrate in drinking water at levels above 10 ppm is a health risk for infants of less than six months of age. High nitrate levels in drinking water can cause blue baby syndrome. Nitrate levels may rise quickly for short periods of time because of rainfall or agricultural activity. If you are caring for an infant, you should ask for advice from your health care provider.
(Above 10 ppm) Infants below the age of six months who drink water containing nitrate in excess of the MCL could become seriously ill and, if untreated, may die. Symptoms include shortness of breath and blue baby syndrome.

	Volatile Organic Contaminants

	Contaminant
(Units)
	Level
Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of
Contamination
	Health Effects of Contaminant

	Haloacetic Acids (HAA)
(ppb)
	     
6.2
	7/2025
	60
	N/A
	No
	By-product of drinking water disinfection
	Some people who drink water containing haloacetic acids in excess of the MCL over many years may have an increased risk of getting cancer.

	Total Trihalomethanes
(TTHM)
(Bromodichloro-methane
Bromoform
Dibromochloro-methane
Chloroform)
(ppb)
	     
6.4
	7/2025
	80
	N/A
	No
	By-product of drinking water chlorination
	Some people who drink water containing trihalomethanes in excess of the MCL over many years may experience problems with their liver, kidneys, or central nervous systems, and may have an increased risk of getting cancer.



	
	
	PER- AND POLYFLUOROALKYL SUBSTANCES (PFAS) CONTAMINANTS

	Contaminant
(Units)

	Level Detected*
	Date
	MCL
	MCLG
	Violation
YES/NO
	Likely Source of Contamination
	Health Effects of Contaminant

	Perfluorohexane sulfonic acid (PFHxS)
(ppt)
	     
.96
	2025
	18
	0
	No
	Discharge from industrial processes, wastewater treatment, residuals from firefighting foam, runoff/leachate from landfills and septic systems.
	Some people who drink water containing perfluorohexane sulfonic acid (PFHxS) in excess of the MCL over many years could experience problems with their liver, endocrine system, or immune system, or may experience increased cholesterol levels. It may also lower a woman’s chance of getting pregnant.

	Perfluorooctane sulfonic acid 
(PFOS)
(ppt)
	1.11

	2025
	15
	0
	     No
	Discharge from industrial processes, wastewater treatment, residuals from firefighting foam, runoff/leachate from landfills and septic systems.
	Some people who drink water containing perfluorooctane sulfonic acid (PFOS) in excess of the MCL over many years could experience problems with their liver, endocrine system, or immune system, may experience increased cholesterol levels, and may have an increased risk of getting certain types of cancer. It may also lower a woman’s chance of getting pregnant.

	Perfluorooctanoic acid (PFOA)
(ppt)
	     
2.08
	2025
	12
	0
	     No
	Discharge from industrial processes, wastewater treatment, residuals from firefighting foam, runoff/leachate from landfills and septic systems.
	Some people who drink water containing perfluorooctanoic acid (PFOA) in excess of the MCL over many years could experience problems with their liver, endocrine system, or immune system, may experience increased cholesterol levels, and may have an increased risk of getting certain types of cancer. It may also lower a woman’s chance of getting pregnant.



	
	
	SECONDARY CONTAMINANTS

	Secondary MCLs (SMCL)

	Level Detected, Average & Range
	Date
	Treatment technique
(if any)
	SMCL 
	50 % AGQS (Ambient groundwater quality standard)
	AGQS (Ambient groundwater quality standard)
	Specific contaminant criteria and reason for monitoring

	Chloride (ppm)
	     
74.5
	2025
	N/A
	250
	N/A
	N/A
	Wastewater, road salt, water softeners, corrosion

	Manganese (ppm)
	.007

	2025
	N/A
	0.05
	0.15
	0.3
	Geological

	pH 
	     
6.8-8.4
	2025
	N/A
	6.5-8.5 (Normal Range)
	N/A
	N/A
	Precipitation and geology

	Sodium (ppm)
	     
54.5
	2025
	N/A
	100-250
	N/A
	N/A
	We are required to regularly sample for sodium

	Sulfate (ppm)
	     
21
	2025
	N/A
	250
	250
	500
	Naturally occurring

	Zinc (ppm)
	     
.0036
	2025
	N/A
	5
	N/A
	N/A
	Galvanized pipes
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